Audio feedback (In an error)

Visual feedback

Check the final output (Book)

Check initial position of the paper tray

Check paper availability

Enter the command to start

Buzzer

5V Relay

Wiper Motor

L298N

12v DC gear Motor

ULN-2003

28BYJ-48

Stepper

A4988

Nema17

LCD Display

**PROCESS**

**OUTPUT**

**Arduino Mega**

**INPUT**

IR Sensor

Limit

Switch

IR Sensor

Keypad